| # Gaudi Framework, version v22r0 |

Home |  | Generated: 9 Feb 2011

# perfmon_dfl_smpl.h

Go to the documentation of this file.

    00001 /*
    00002  * Copyright (c) 2005-2006 Hewlett-Packard Development Company, L.P.
    00003  *               Contributed by Stephane Eranian <eranian@hpl.hp.com>
    00004  *
    00005  * This file implements the new dfl sampling buffer format
    00006  * for perfmon2 subsystem.
    00007  *
    00008  * This format is supported used by all platforms. For IA-64, older
    00009  * applications using perfmon v2.0 MUST use the
    00010  * perfmon_default_smpl.h
    00011  */
    00012 #ifndef __PERFMON_DFL_SMPL_H__
    00013 #define __PERFMON_DFL_SMPL_H__ 1
    00014
    00015 #ifdef __cplusplus
    00016 extern "C" {
    00017 #endif
    00018
    00019 #include <perfmon/perfmon.h>
    00020
    00021 #define PFM_DFL_SMPL_NAME       "default"
    00022
    00023 #ifdef PFMLIB_OLD_PFMV2
    00024 /*
    00025  * UUID for compatibility with perfmon v2.2 (used by Cray)
    00026  */
    00027 #define PFM_DFL_SMPL_UUID { \
    00028        0xd1, 0x39, 0xb2, 0x9e, 0x62, 0xe8, 0x40, 0xe4,\
    00029        0xb4, 0x02, 0x73, 0x07, 0x87, 0x92, 0xe9, 0x37 }
    00030 #endif
    00031
    00032 /*
    00033  * format specific parameters (passed at context creation)
    00034  */
    00035 typedef struct {
    00036         uint64_t        buf_size;       /* size of the buffer in bytes */
    00037         uint32_t        buf_flags;      /* buffer specific flags */
    00038         uint32_t        res1;           /* for future use */
    00039         uint64_t        reserved[6];    /* for future use */
    00040 } pfm_dfl_smpl_arg_t;
    00041
    00042 /*
    00043  * This header is at the beginning of the sampling buffer returned to the user.
    00044  * It is directly followed by the first record.
    00045  */
    00046 typedef struct {
    00047         uint64_t        hdr_count;              /* how many valid entries */
    00048         uint64_t        hdr_cur_offs;           /* current offset from top of buffer */
    00049         uint64_t        hdr_overflows;          /* #overflows for buffer */
    00050         uint64_t        hdr_buf_size;           /* bytes in the buffer */
    00051         uint64_t        hdr_min_buf_space;      /* minimal buffer size (internal use) */
    00052         uint32_t        hdr_version;            /* smpl format version */
    00053         uint32_t        hdr_buf_flags;          /* copy of buf_flags */
    00054         uint64_t        hdr_reserved[10];       /* for future use */
    00055 } pfm_dfl_smpl_hdr_t;
    00056
    00057 /*
    00058  * Entry header in the sampling buffer.  The header is directly followed
    00059  * with the values of the PMD registers of interest saved in increasing
    00060  * index order: PMD4, PMD5, and so on. How many PMDs are present depends
    00061  * on how the session was programmed.
    00062  *
    00063  * In the case where multiple counters overflow at the same time, multiple
    00064  * entries are written consecutively.
    00065  *
    00066  * last_reset_value member indicates the initial value of the overflowed PMD.
    00067  */
    00068 typedef struct {
    00069         uint32_t        pid;                    /* thread id (for NPTL, this is gettid()) */
    00070         uint16_t        ovfl_pmd;               /* index of pmd that overflowed for this sample */
    00071         uint16_t        reserved;               /* for future use */
    00072         uint64_t        last_reset_val;         /* initial value of overflowed PMD */
    00073         uint64_t        ip;                     /* where did the overflow interrupt happened  */
    00074         uint64_t        tstamp;                 /* overflow timetamp */
    00075         uint16_t        cpu;                    /* cpu on which the overfow occured */
    00076         uint16_t        set;                    /* event set active when overflow ocurred   */
    00077         uint32_t        tgid;                   /* thread group id (for NPTL, this is getpid()) */
    00078 } pfm_dfl_smpl_entry_t;
    00079
    00080 #define PFM_DFL_SMPL_VERSION_MAJ        1U
    00081 #define PFM_DFL_SMPL_VERSION_MIN        0U
    00082 #define PFM_DFL_SMPL_VERSION    (((PFM_DFL_SMPL_VERSION_MAJ&0xffff)<<16)|(PFM_DFL_SMPL_VERSION_MIN & 0xffff))
    00083
    00084 #ifdef __cplusplus
    00085 };
    00086 #endif
    00087
    00088 #endif /* __PERFMON_DFL_SMPL_H__ */

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Properties Friends Defines