| # Gaudi Framework, version v22r4 |

Home |  | Generated: Fri Sep 2 2011

# perfmon_pebs_p4_smpl.h

Go to the documentation of this file.

    00001 /*
    00002  * Copyright (c) 2005-2007 Hewlett-Packard Development Company, L.P.
    00003  *               Contributed by Stephane Eranian <eranian@hpl.hp.com>
    00004  *
    00005  * This program is free software; you can redistribute it and/or
    00006  * modify it under the terms of version 2 of the GNU General Public
    00007  * License as published by the Free Software Foundation.
    00008  *
    00009  * This program is distributed in the hope that it will be useful,
    00010  * but WITHOUT ANY WARRANTY; without even the implied warranty of
    00011  * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU
    00012  * General Public License for more details.
    00013  *
    00014  * You should have received a copy of the GNU General Public License
    00015  * along with this program; if not, write to the Free Software
    00016  * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA
    00017  * 02111-1307 USA
    00018  *
    00019  * This file implements the sampling format to support Intel
    00020  * Precise Event Based Sampling (PEBS) feature of Pentium 4
    00021  * and other Netburst-based processors. Not to be used for
    00022  * Intel Core-based processors.
    00023  *
    00024  * What is PEBS?
    00025  * ------------
    00026  *  This is a hardware feature to enhance sampling by providing
    00027  *  better precision as to where a sample is taken. This avoids the
    00028  *  typical skew in the instruction one can observe with any
    00029  *  interrupt-based sampling technique.
    00030  *
    00031  *  PEBS also lowers sampling overhead significantly by having the
    00032  *  processor store samples instead of the OS. PMU interrupt are only
    00033  *  generated after multiple samples are written.
    00034  *
    00035  *  Another benefit of PEBS is that samples can be captured inside
    00036  *  critical sections where interrupts are masked.
    00037  *
    00038  * How does it work?
    00039  *  PEBS effectively implements a Hw buffer. The Os must pass a region
    00040  *  of memory where samples are to be stored. The region can have any
    00041  *  size. The OS must also specify the sampling period to reload. The PMU
    00042  *  will interrupt when it reaches the end of the buffer or a specified
    00043  *  threshold location inside the memory region.
    00044  *
    00045  *  The description of the buffer is stored in the Data Save Area (DS).
    00046  *  The samples are stored sequentially in the buffer. The format of the
    00047  *  buffer is fixed and specified in the PEBS documentation.  The sample
    00048  *  format changes between 32-bit and 64-bit modes due to extended register
    00049  *  file.
    00050  *
    00051  *  PEBS does not work when HyperThreading is enabled due to certain MSR
    00052  *  being shared being to two threads.
    00053  *
    00054  *  What does the format do?
    00055  *   It provides access to the PEBS feature for both 32-bit and 64-bit
    00056  *   processors that support it.
    00057  *
    00058  *   The same code is used for both 32-bit and 64-bit modes, but different
    00059  *   format names are used because the two modes are not compatible due to
    00060  *   data model and register file differences. Similarly the public data
    00061  *   structures describing the samples are different.
    00062  *
    00063  *   It is important to realize that the format provides a zero-copy environment
    00064  *   for the samples, i.e,, the OS never touches the samples. Whatever the
    00065  *   processor write is directly accessible to the user.
    00066  *
    00067  *   Parameters to the buffer can be passed via pfm_create_context() in
    00068  *   the pfm_pebs_smpl_arg structure.
    00069  *
    00070  *   It is not possible to mix a 32-bit PEBS application on top of a 64-bit
    00071  *   host kernel.
    00072  */
    00073 #ifndef __PERFMON_PEBS_P4_SMPL_H__
    00074 #define __PERFMON_PEBS_P4_SMPL_H__ 1
    00075
    00076 #ifdef __cplusplus
    00077 extern "C" {
    00078 #endif
    00079
    00080 #include <perfmon/perfmon.h>
    00081
    00082 #ifdef __i386__
    00083 #define PFM_PEBS_P4_SMPL_NAME   "pebs32_p4"
    00084 #else
    00085 #define PFM_PEBS_P4_SMPL_NAME   "pebs64_p4"
    00086 #endif
    00087
    00088 /*
    00089  * format specific parameters (passed at context creation)
    00090  */
    00091 typedef struct {
    00092         uint64_t        cnt_reset;      /* counter reset value */
    00093         size_t          buf_size;       /* size of the buffer in bytes */
    00094         size_t          intr_thres;     /* index of interrupt threshold entry */
    00095         uint64_t        reserved[6];    /* for future use */
    00096 } pfm_pebs_p4_smpl_arg_t;
    00097
    00098 /*
    00099  * DS Save Area as described in section 15.10.5
    00100  */
    00101 typedef struct {
    00102         unsigned long   bts_buf_base;
    00103         unsigned long   bts_index;
    00104         unsigned long   bts_abs_max;
    00105         unsigned long   bts_intr_thres;
    00106         unsigned long   pebs_buf_base;
    00107         unsigned long   pebs_index;
    00108         unsigned long   pebs_abs_max;
    00109         unsigned long   pebs_intr_thres;
    00110         uint64_t        pebs_cnt_reset;
    00111 } pfm_ds_area_p4_t;
    00112
    00113 /*
    00114  * This header is at the beginning of the sampling buffer returned to the user.
    00115  *
    00116  * Because of PEBS alignement constraints, the actual PEBS buffer area does
    00117  * not necessarily begin right after the header. The hdr_start_offs must be
    00118  * used to compute the first byte of the buffer. The offset is defined as
    00119  * the number of bytes between the end of the header and the beginning of
    00120  * the buffer. As such the formula is:
    00121  *      actual_buffer = (unsigned long)(hdr+1)+hdr->hdr_start_offs
    00122  */
    00123 typedef struct {
    00124         uint64_t                overflows;      /* #overflows for buffer */
    00125         size_t                  buf_size;       /* bytes in the buffer */
    00126         size_t                  start_offs;     /* actual buffer start offset */
    00127         uint32_t                version;        /* smpl format version */
    00128         uint32_t                reserved1;      /* for future use */
    00129         uint64_t                reserved2[5];   /* for future use */
    00130         pfm_ds_area_p4_t        ds;             /* DS management Area */
    00131 } pfm_pebs_p4_smpl_hdr_t;
    00132
    00133 /*
    00134  * PEBS record format as for both 32-bit and 64-bit modes
    00135  */
    00136 typedef struct {
    00137         unsigned long eflags;
    00138         unsigned long ip;
    00139         unsigned long eax;
    00140         unsigned long ebx;
    00141         unsigned long ecx;
    00142         unsigned long edx;
    00143         unsigned long esi;
    00144         unsigned long edi;
    00145         unsigned long ebp;
    00146         unsigned long esp;
    00147 #ifdef __x86_64__
    00148         unsigned long r8;
    00149         unsigned long r9;
    00150         unsigned long r10;
    00151         unsigned long r11;
    00152         unsigned long r12;
    00153         unsigned long r13;
    00154         unsigned long r14;
    00155         unsigned long r15;
    00156 #endif
    00157 } pfm_pebs_p4_smpl_entry_t;
    00158
    00159 #define PFM_PEBS_P4_SMPL_VERSION_MAJ 1U
    00160 #define PFM_PEBS_P4_SMPL_VERSION_MIN 0U
    00161 #define PFM_PEBS_P4_SMPL_VERSION (((PFM_PEBS_P4_SMPL_VERSION_MAJ&0xffff)<<16)|\
    00162                                    (PFM_PEBS_P4_SMPL_VERSION_MIN & 0xffff))
    00163
    00164 #ifdef __cplusplus
    00165 };
    00166 #endif
    00167
    00168 #endif /* __PERFMON_PEBS_P4_SMPL_H__ */

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Properties Friends Defines