| # Gaudi Framework, version v23r1 |

Home |  | Generated: Wed Feb 29 2012

# pfmlib_pentium4.h

Go to the documentation of this file.

    00001 /*
    00002  * Intel Pentium 4 PMU specific types and definitions (32 and 64 bit modes)
    00003  *
    00004  * Copyright (c) 2006 IBM Corp.
    00005  * Contributed by Kevin Corry <kevcorry@us.ibm.com>
    00006  *
    00007  * Permission is hereby granted, free of charge, to any person obtaining a copy
    00008  * of this software and associated documentation files (the "Software"), to deal
    00009  * in the Software without restriction, including without limitation the rights
    00010  * to use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies
    00011  * of the Software, and to permit persons to whom the Software is furnished to do so,
    00012  * subject to the following conditions:
    00013  *
    00014  * The above copyright notice and this permission notice shall be included in all
    00015  * copies or substantial portions of the Software.
    00016  *
    00017  * THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED,
    00018  * INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A
    00019  * PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
    00020  * HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF
    00021  * CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE
    00022  * OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
    00023  */
    00024
    00025 #ifndef __PFMLIB_PENTIUM4_H__
    00026 #define __PFMLIB_PENTIUM4_H__
    00027
    00028 #include <perfmon/pfmlib.h>
    00029
    00030 /* ESCR: Event Selection Control Register
    00031  *
    00032  * These registers are used to select which event to count along with options
    00033  * for that event. There are (up to) 45 ESCRs, but each data counter is
    00034  * restricted to a specific set of ESCRs.
    00035  */
    00036
    00055 #define EVENT_MASK_BITS 16
    00056 #define EVENT_SELECT_BITS 6
    00057
    00058 typedef union {
    00059         unsigned long val;
    00060         struct {
    00061                 unsigned long t1_usr:1;
    00062                 unsigned long t1_os:1;
    00063                 unsigned long t0_usr:1;
    00064                 unsigned long t0_os:1;
    00065                 unsigned long tag_enable:1;
    00066                 unsigned long tag_value:4;
    00067                 unsigned long event_mask:EVENT_MASK_BITS;
    00068                 unsigned long event_select:EVENT_SELECT_BITS;
    00069                 unsigned long reserved:1;
    00070         } bits;
    00071 } pentium4_escr_value_t;
    00072
    00073 /* CCCR: Counter Configuration Control Register
    00074  *
    00075  * These registers are used to configure the data counters. There are 18
    00076  * CCCRs, one for each data counter.
    00077  */
    00078
    00111 typedef union {
    00112         unsigned long val;
    00113         struct {
    00114                 unsigned long reserved1:12;
    00115                 unsigned long enable:1;
    00116                 unsigned long escr_select:3;
    00117                 unsigned long active_thread:2;
    00118                 unsigned long compare:1;
    00119                 unsigned long complement:1;
    00120                 unsigned long threshold:4;
    00121                 unsigned long edge:1;
    00122                 unsigned long force_ovf:1;
    00123                 unsigned long ovf_pmi_t0:1;
    00124                 unsigned long ovf_pmi_t1:1;
    00125                 unsigned long reserved2:2;
    00126                 unsigned long cascade:1;
    00127                 unsigned long overflow:1;
    00128         } bits;
    00129 } pentium4_cccr_value_t;
    00130
    00131 #endif /* __PFMLIB_PENTIUM4_H__ */

All Classes Namespaces Files Functions Variables Typedefs Enumerations Enumerator Properties Friends Defines