| The Gaudi Framework v28r2-patches (bc4ad17a)

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Public Attributes | List of all members
pentium4_cccr_value_t Union Reference

pentium4_cccr_value_t More...

`#include <src/component/perfmon/pfmlib_pentium4.h>`

## Public Attributes
unsigned long | val
struct {
unsigned long reserved1:12
unsigned long enable:1
unsigned long escr_select:3
unsigned long active_thread:2
unsigned long compare:1
unsigned long complement:1
unsigned long threshold:4
unsigned long edge:1
unsigned long force_ovf:1
unsigned long ovf_pmi_t0:1
unsigned long ovf_pmi_t1:1
unsigned long reserved2:2
unsigned long cascade:1
unsigned long overflow:1
} | bits

## Detailed Description

pentium4_cccr_value_t

Bit-wise breakdown of the CCCR registers.

Bits Description

63 - 32 Reserved 31 OVF - The data counter overflowed. 30 Cascade - Enable cascading of data counter when alternate counter overflows. 29 - 28 Reserved 27 OVF_PMI_T1 - Generate interrupt for LP1 on counter overflow 26 OVF_PMI_T0 - Generate interrupt for LP0 on counter overflow 25 FORCE_OVF - Force interrupt on every counter increment 24 Edge - Enable rising edge detection of the threshold comparison output for filtering event counts. 23 - 20 Threshold Value - Select the threshold value for comparing to incoming event counts. 19 Complement - Select how incoming event count is compared with the threshold value. 18 Compare - Enable filtering of event counts. 17 - 16 Active Thread - Only used with HT enabled. 00 - None: Count when neither LP is active. 01 - Single: Count when only one LP is active. 10 - Both: Count when both LPs are active. 11 - Any: Count when either LP is active. 15 - 13 ESCR Select - Select which ESCR to use for selecting the event to count. 12 Enable - Turns the data counter on or off. 11 - 0 Reserved

Definition at line 111 of file pfmlib_pentium4.h.

## Member Data Documentation

unsigned long pentium4_cccr_value_t::active_thread

Definition at line 117 of file pfmlib_pentium4.h.

struct { ... } pentium4_cccr_value_t::bits

unsigned long pentium4_cccr_value_t::cascade

Definition at line 126 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::compare

Definition at line 118 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::complement

Definition at line 119 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::edge

Definition at line 121 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::enable

Definition at line 115 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::escr_select

Definition at line 116 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::force_ovf

Definition at line 122 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::overflow

Definition at line 127 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::ovf_pmi_t0

Definition at line 123 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::ovf_pmi_t1

Definition at line 124 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::reserved1

Definition at line 114 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::reserved2

Definition at line 125 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::threshold

Definition at line 120 of file pfmlib_pentium4.h.

unsigned long pentium4_cccr_value_t::val

Definition at line 112 of file pfmlib_pentium4.h.

The documentation for this union was generated from the following file:

- GaudiProfiling/src/component/perfmon/pfmlib_pentium4.h