| The Gaudi Framework v29r1 (5cd95fa2)

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- File List
- File Members

instrset_detect.cpp
Go to the documentation of this file.
1 /************************** instrset_detect.cpp ****************************
2 * Author: Agner Fog
3 * Date created: 2012-05-30
4 * Last modified: 2017-05-02
5 * Version: 1.28
6 * Project: vector classes
7 * Description:
8 * Functions for checking which instruction sets are supported.
9 *
10 * (c) Copyright 2012-2017 GNU General Public License http://www.gnu.org/licenses
11 \*****************************************************************************/
12
13 #include "instrset.h"
14
15 #ifdef VCL_NAMESPACE
16 namespace VCL_NAMESPACE
17 {
18 #endif
19
20 // Define interface to cpuid instruction.
21 // input: eax = functionnumber, ecx = 0
22 // output: eax = output[0], ebx = output[1], ecx = output[2], edx = output[3]
23 static inline void cpuid( int output[4], int functionnumber )
24 {
25 #if defined( __GNUC__ ) || defined( __clang__ ) // use inline assembly, Gnu/AT&T syntax
26
27 int a, b, c, d;
28 __asm( "cpuid" : "=a"( a ), "=b"( b ), "=c"( c ), "=d"( d ) : "a"( functionnumber ), "c"( 0 ) : );
29 output[0] = a;
30 output[1] = b;
31 output[2] = c;
32 output[3] = d;
33
34 #elif defined( _MSC_VER ) || defined( __INTEL_COMPILER ) // Microsoft or Intel compiler, intrin.h included
35
36 __cpuidex( output, functionnumber, 0 ); // intrinsic function for CPUID
37
38 #else // unknown platform. try inline assembly with masm/intel syntax
39
40 __asm {
41 mov eax, functionnumber
42 xor ecx, ecx
43 cpuid;
44 mov esi, output
45 mov [esi], eax
46 mov [esi+4], ebx
47 mov [esi+8], ecx
48 mov [esi+12], edx
49 }
50
51 #endif
52 }
53
54 // Define interface to xgetbv instruction
55 static inline int64_t xgetbv( int ctr )
56 {
57 #if ( defined( _MSC_FULL_VER ) && _MSC_FULL_VER >= 160040000 ) || \
58 ( defined( __INTEL_COMPILER ) && \
59 __INTEL_COMPILER >= 1200 ) // Microsoft or Intel compiler supporting _xgetbv intrinsic
60
61 return _xgetbv( ctr ); // intrinsic function for XGETBV
62
63 #elif defined( __GNUC__ ) // use inline assembly, Gnu/AT&T syntax
64
65 uint32_t a, d;
66 __asm( "xgetbv" : "=a"( a ), "=d"( d ) : "c"( ctr ) : );
67 return a | ( uint64_t( d ) << 32 );
68
69 #else // #elif defined (_WIN32) // other compiler. try inline assembly with masm/intel/MS
70 // syntax
71
72 uint32_t a, d;
73 __asm {
74 mov ecx, ctr
75 _emit 0x0f
76 _emit 0x01
77 _emit 0xd0 ; // xgetbv
78 mov a, eax
79 mov d, edx
80 }
81 return a | ( uint64_t( d ) << 32 );
82
83 #endif
84 }
85
86 /* find supported instruction set
87 return value:
88 0 = 80386 instruction set
89 1 or above = SSE (XMM) supported by CPU (not testing for O.S. support)
90 2 or above = SSE2
91 3 or above = SSE3
92 4 or above = Supplementary SSE3 (SSSE3)
93 5 or above = SSE4.1
94 6 or above = SSE4.2
95 7 or above = AVX supported by CPU and operating system
96 8 or above = AVX2
97 9 or above = AVX512F
98 10 or above = AVX512VL
99 11 or above = AVX512BW, AVX512DQ
100 */
101 int instrset_detect( void )
102 {
103
104 static int iset = -1; // remember value for next call
105 if ( iset >= 0 ) {
106 return iset; // called before
107 }
108 iset = 0; // default value
109 int abcd[4] = {0, 0, 0, 0}; // cpuid results
110 cpuid( abcd, 0 ); // call cpuid function 0
111 if ( abcd[0] == 0 ) return iset; // no further cpuid function supported
112 cpuid( abcd, 1 ); // call cpuid function 1 for feature flags
113 if ( ( abcd[3] & ( 1 << 0 ) ) == 0 ) return iset; // no floating point
114 if ( ( abcd[3] & ( 1 << 23 ) ) == 0 ) return iset; // no MMX
115 if ( ( abcd[3] & ( 1 << 15 ) ) == 0 ) return iset; // no conditional move
116 if ( ( abcd[3] & ( 1 << 24 ) ) == 0 ) return iset; // no FXSAVE
117 if ( ( abcd[3] & ( 1 << 25 ) ) == 0 ) return iset; // no SSE
118 iset = 1; // 1: SSE supported
119 if ( ( abcd[3] & ( 1 << 26 ) ) == 0 ) return iset; // no SSE2
120 iset = 2; // 2: SSE2 supported
121 if ( ( abcd[2] & ( 1 << 0 ) ) == 0 ) return iset; // no SSE3
122 iset = 3; // 3: SSE3 supported
123 if ( ( abcd[2] & ( 1 << 9 ) ) == 0 ) return iset; // no SSSE3
124 iset = 4; // 4: SSSE3 supported
125 if ( ( abcd[2] & ( 1 << 19 ) ) == 0 ) return iset; // no SSE4.1
126 iset = 5; // 5: SSE4.1 supported
127 if ( ( abcd[2] & ( 1 << 23 ) ) == 0 ) return iset; // no POPCNT
128 if ( ( abcd[2] & ( 1 << 20 ) ) == 0 ) return iset; // no SSE4.2
129 iset = 6; // 6: SSE4.2 supported
130 if ( ( abcd[2] & ( 1 << 27 ) ) == 0 ) return iset; // no OSXSAVE
131 if ( ( xgetbv( 0 ) & 6 ) != 6 ) return iset; // AVX not enabled in O.S.
132 if ( ( abcd[2] & ( 1 << 28 ) ) == 0 ) return iset; // no AVX
133 iset = 7; // 7: AVX supported
134 cpuid( abcd, 7 ); // call cpuid leaf 7 for feature flags
135 if ( ( abcd[1] & ( 1 << 5 ) ) == 0 ) return iset; // no AVX2
136 iset = 8;
137 if ( ( abcd[1] & ( 1 << 16 ) ) == 0 ) return iset; // no AVX512
138 cpuid( abcd, 0xD ); // call cpuid leaf 0xD for feature flags
139 if ( ( abcd[0] & 0x60 ) != 0x60 ) return iset; // no AVX512
140 iset = 9;
141 cpuid( abcd, 7 ); // call cpuid leaf 7 for feature flags
142 if ( ( abcd[1] & ( 1 << 31 ) ) == 0 ) return iset; // no AVX512VL
143 iset = 10;
144 if ( ( abcd[1] & 0x40020000 ) != 0x40020000 ) return iset; // no AVX512BW, AVX512DQ
145 iset = 11;
146 return iset;
147 }
148
149 // detect if CPU supports the FMA3 instruction set
150 bool hasFMA3( void )
151 {
152 if ( instrset_detect() < 7 ) return false; // must have AVX
153 int abcd[4]; // cpuid results
154 cpuid( abcd, 1 ); // call cpuid function 1
155 return ( ( abcd[2] & ( 1 << 12 ) ) != 0 ); // ecx bit 12 indicates FMA3
156 }
157
158 // detect if CPU supports the FMA4 instruction set
159 bool hasFMA4( void )
160 {
161 if ( instrset_detect() < 7 ) return false; // must have AVX
162 int abcd[4]; // cpuid results
163 cpuid( abcd, 0x80000001 ); // call cpuid function 0x80000001
164 return ( ( abcd[2] & ( 1 << 16 ) ) != 0 ); // ecx bit 16 indicates FMA4
165 }
166
167 // detect if CPU supports the XOP instruction set
168 bool hasXOP( void )
169 {
170 if ( instrset_detect() < 7 ) return false; // must have AVX
171 int abcd[4]; // cpuid results
172 cpuid( abcd, 0x80000001 ); // call cpuid function 0x80000001
173 return ( ( abcd[2] & ( 1 << 11 ) ) != 0 ); // ecx bit 11 indicates XOP
174 }
175
176 // detect if CPU supports the F16C instruction set
177 bool hasF16C( void )
178 {
179 if ( instrset_detect() < 7 ) return false; // must have AVX
180 int abcd[4]; // cpuid results
181 cpuid( abcd, 1 ); // call cpuid function 1
182 return ( ( abcd[2] & ( 1 << 29 ) ) != 0 ); // ecx bit 29 indicates F16C
183 }
184
185 // detect if CPU supports the AVX512ER instruction set
186 bool hasAVX512ER( void )
187 {
188 if ( instrset_detect() < 9 ) return false; // must have AVX512F
189 int abcd[4]; // cpuid results
190 cpuid( abcd, 7 ); // call cpuid function 7
191 return ( ( abcd[1] & ( 1 << 27 ) ) != 0 ); // ebx bit 27 indicates AVX512ER
192 }
193
194 #ifdef VCL_NAMESPACE
195 }
196 #endif
VCL_NAMESPACE
#define VCL_NAMESPACE
Definition: System.cpp:27
hasF16C
bool hasF16C(void)
Definition: instrset_detect.cpp:177
hasXOP
bool hasXOP(void)
Definition: instrset_detect.cpp:168
gaudirun.c
c
Definition: gaudirun.py:407
instrset.h
gaudirun.output
output
Definition: gaudirun.py:404
instrset_detect
int instrset_detect(void)
Definition: instrset_detect.cpp:101
uint64_t
unsigned long long uint64_t
Definition: instrset.h:143
hasFMA4
bool hasFMA4(void)
Definition: instrset_detect.cpp:159
int64_t
long long int64_t
Definition: instrset.h:142
hasAVX512ER
bool hasAVX512ER(void)
Definition: instrset_detect.cpp:186
uint32_t
unsigned int uint32_t
Definition: instrset.h:141
cpuid
#define cpuid(func, eax, ebx, ecx, edx)
Definition: PfmCodeAnalyser.h:20
hasFMA3
bool hasFMA3(void)
Definition: instrset_detect.cpp:150